|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5 | 4 | 3 | 2 | 1 |
| You followed all of the preparation steps correctly.  | You followed all of the preparation steps, but your material was not square.  | Your piece had glue on it still but was square.  | Your piece had glue on it and was not square.  | You just put some wood on the lathe did not follow prep steps.  |
| Your piece was sanded nicely. There were no sanding marks or machining marks.  | There were visable sanding marks.  | There were visable sanding and machining marks.  | The piece was really rough and had several machining and sanding marks.  | The piece was not sanded at all.  |
| Your piece was drilled correctly and the season holes were centered. | Your season holes was not centered, but there were not marks in the top of the call from the drill bit.  | You scratched up the top of the shaker with the drill bit, but the hole was centered.  | You scratched up the top of the shaker as well as the hole not being centered.  | You did not drill the shaker holes.  |
| You finished your piece and it had at least 2 even coats.  | You finished your piece and it had one coat, or one coat of wax. | You put one coat of finish on but it was not even.  | You put only wax on it and it was not even. | You did not finish the piece.  |

\_\_\_\_\_\_\_\_ / 20

Comments: